


VT1000 64GB SD

SD CARD SUPPORT

STEPS

* Check Current version of PC viewer and VT1000 Firmware
* Download the latest PC viewer 1.0.8.0 from (LINK) [Support.visiontrack.com](https://support.visiontrack.com/)
* Download the latest VT1000 firmware 1.1.4 (LINK) [Support.visiontrack.com](https://support.visiontrack.com/)
* Install PC viewer
* Copy firmware to SD card
* Insert SD card into VT1000 (Firmware upgrade)
* Leave recording for a few minutes then check SD card back in PC viewer to confirm firmware has applied
* Initialise SD card, check and change settings and put back into VT1000

1

* Check current firmware and PC viewer version
* Remove SD card from VT1000
* Insert into PC and open PC viewer software
* Click on 
* Select the SD card 
* Select the  icon
* This will show you the current PC viewer and Firmware installed on the VT1000 

2


* If required, download the latest PC viewer 1.0.8.0 from ([LINK](https://support.visiontrack.com/a/solutions/articles/76000014217)) support.visiontrack.com
* Remove the old version from your PC and install the latest version.

3

* If required download the latest VT1000 firmware 1.1.4 ([LINK](https://support.visiontrack.com/a/solutions/articles/76000014391)) support.visiontrack.com
* Download the zip file and unzip the folder, move the folder (program) to the root of the VT1000 SD card.


4



* Firmware upgrade  
  **(DO NOT TURN THE POWER OFF DURING THE UPGRADE AS THIS WILL CASUE THE UNIT TO FAIL)**
* Put the SD card into the VT1000.  
  The VT1000 will flash red and blue at the same time for a few seconds and then reboot.
* Once complete the VT1000 will show the blue LED, press the panic button and leave the unit recording for a few minutes.
* Turn off the VT1000 and put the SD card back into the PC viewer.
* Follow step 1 to check the firmware has applied



5

* Initialise SD, check and change settings
* Click on 
* Click on Init SD Card 
* Select ‘Quick Format’ and remove the tick from ‘Backup Configuration File’ and click start



* Once initialised
* Change any settings you need to, **PLEASE MAKE SURE THE TICK IS REMOVED FROM SD CARD AUTO FORMAT FEATURE**
* Click on ‘OK’
* Select ‘OK’ to save current settings 
* You can now remove the SD card and place this back into the VT1000.



support.visiontrack.com

Need Support?